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TERMS & CONDITIONS

FOR

PURCHASES / PROCUREMENTS UNDER TENDERING / BIDDING
	Firm Name:
	
	
	
	
	

	M/s_______________________________________________________________________________

	Proprietor Name:_______________________________
	CNIC #.________________________________

	NTN #:___________________________
	Sales Tax #.___________________________

	Address:____________________________________________________________________________

	Ph #:_________________   Cell # ​​​​​________________________
	
	
	
	
	


General Terms and Conditions

i. Any offer which is not received as per terms and conditions of the tender enquiry is liable to be ignored. No offer shall be considered if: 

a. Received without earnest money.

b. It is received after the time and date fixed for its receipt.

c. The tender is unsigned

d. The offer is ambiguous

e. The offer is conditional

f. The offer is from a black listed firm.

g. The offer is received by fax or e-mail

h. Offer received with shorter validity than required.

i. The offer is not conforming to specifications indicated in the tender enquiry.

j. The tender documents are not signed by the supplier or his authorized person(s).

ii. Offer must remain valid for at least 30 days from the date of opening the tender.

iii. The covering letter should indicate particulars of tender, and date of opening. The envelope must be properly sealed.

iv. The purchaser reserves the rights to purchase full or part or ignore / scrap / cancel the tender without assigning any reason(s). The earnest money / security shall be forfeited if:

a. The acceptance of tender is not issued during the validity period by the successful bidder within stipulated time period. 

b. The offer is withdrawn, amended or revised during the validity period of the offer without approval of the buyer.

c. The contractor fails to execute the contract strictly in accordance with term and condition of the tender.

v. The Bidder shall enclose catalogues / leaflets / literature and other technical information, if any, in respect of items offered by him. 
vi. The contractor will be responsible for the free replacement of items if the same is found to be substandard by the purchaser and or at variance with the specifications given in the tender enquiry. Items offered of a specification superior to the one specified in the tender enquiry may be accepted by the purchaser.

vii. Where offers have been invited for specified quality, offers of other quality shall not be acceptable.

viii. Items should be brand new and in original manufacturers packing.

ix. Inverter and Batteries should covered 2 years replacement warranty and solar panels replacement warranty period must be 10 years. 

x. The Bidder should indicate their National Income Tax & Sales Tax Number.

xi. The Bidder will produce documents if required by purchaser to ensure that store supplied is brand new and in original packing of manufacturer.

xii. The quoted price should clearly indicate whether it includes taxes or not.

xiii. The purchaser is entitled to deduct all prevailing taxes.  
2-
Technical Advice

i.
Bidder will have to provide distribution certificate of foreign Principle.

ii
Purchase Committee will examine to bidders Stock/Warehouse.
iii
The CCRI, Multan may seek technical advice for vetting tender offers from any person having appropriate knowledge/experience in the relevant field.

3- 
Evaluation Criteria 

Bids will be evaluated in terms of technically and financially. The Purchaser has the liberty to reject the lowest bidder if the quoted material has been found the low quality and not fulfilling the required results, which are expected for better quality results.
4-
Delivery of Items.
Delivery of Items must be insured within 15 days after purchase order.


5-
Inspection of Items 
Inspection of the delivered item shall be conducted by purchase committee, which has a technical member especially for this particular purchase, before its acceptance.

6-
Payment to the Contractors

i. Payment of the amount will be made through crossed cheques to the supplier against invoice submitted to the Project Manager, PBW Project CCRI, Multan after 100% completion of delivery, installation / commissioning and satisfactory performance. Chairman Purchase committee /Project Manager, PBW Project Central Cotton Research Institute, Multan will determine the status of the completion of supply and issue instructions for payment.

ii. Payment against partial supply will not be made until goods have been received & satisfactory report has been generated.

7- Earnest Money

Earnest money @ 2% of the tender value will have to be deposited along with tender. It should be in the form of Bank Draft/Call Deposit in favor of Project Manager, PBW Project Central Cotton Research Institute, Multan.
Earnest money shall be refunded on successful completion of the contract. The earnest money furnished by the firm may be retained for adjustment of the amount due against the firm in case, the said firm is defaulter against any other contract.

8-
Deduction of Taxes

Income and other taxes will be deducted while making payment as per most recent Government instructions / notifications.

9-
Payment of Sales and other Taxes

Purchase should be made from the firms registered with sale & income tax departments.

10-
Security money

10% of all the awarded contract money will retain by the buyer for the period of warranty period.

11-
Termination of Contract
The Director CCRI/Project Manager PBW Project on the recommendation of the purchase committee may terminate this supply order for valid reasons and will inform the supplier about his decision in writing.

12-        Submission of Tender

Last date of submission of the tender is 06.01.2022 in the office of the Director Central Cotton Research Institute, Multan 

13-      Opening of Tender

Date of opening the tender is 06.01.2022 in the office of the Director Central Cotton Research Institute, Multan. Tender will be opened in the presence of all parties/their representatives.

14-
Purchas Committee decision will be Final. 
   Signature & Stamp
Of Supplier
List of items required for Project titled: "Cotton Productivity Enhancement Trough Eco-Friendly Pink Bollworm Management and Capacity Building PM Emergency Program"

	Sr.No.
	Name of Items
	Quantity

	1.
	Pink Bollworm Machines
	02 Nos.

	2.
	Solar System (25KW)
	01 No.

	3.
	Laboratory Refrigerator (2 – 8oC)
	01 No.

	4.
	Laboratory Refrigerator (-20oC)
	01 No.

	5.
	Laminar Air Flow Cabinet
	01 No.

	6.
	Temperature Controlled Shaking Incubator
	01 No.

	7.
	Ultra Pure (miliQ) Water Purification System
	01 No.

	8.
	Gel Documentation System
	01 No.

	9.
	CI-340 -Handheld Photosynthesis system
	01 No.

	10.
	CCL-DZ-10Z Water Distiller (chinacaremedical.com)
	01 No.

	11.
	Olympus SZX7 Stereo Microscope
	01 No.

	12.
	Nikon SMZ745 Stereo Microscope
	01 No.

	13.
	Canon EOS 6D Mark II DSLR Camera
	01 No.

	14.
	Nikon Microscope ECLIPSE Ci-E
	01 No.


Note: 
Quantity of items may vary and will be finalized at the time of placing order subject to availability of funds

TECHNICAL SPACIFICATION:
PINK BOLLWORM MANAGER (MECHANICAL BOLL PICKER)
GENERAL

	1. Type
	Tractor Rear Mounted 

	2. Application
	For stripping the cotton bolls to eliminate the disease 

	3. Working width 
	2650

	4. Universal shaft
	Improved quality with protective cover 

	5. Nos of stripper 
	04

	6. Hydraulic operation 
	With tractor hydraulic system.

	7. Tractor compatibility 
	 75 hp and above 


OVERALL DIMENSIONS

	8. Overall width
	3050  mm ± 50mm

	9. Working width
	2690  mm ± 50mm

	10. Front two back length
	4000  mm ± 50mm

	11. Height
	3150  mm ± 50mm


MATERIAL SPECIFICATIONS 

	12. Main frame  
	M.S angle box 50 x 6mm,  38x6mm, MS channel 80x40x6mm 

	13. Gear box and main driving shaft 
	MS shaft 28.5 mm dia attached with main frame MS angle box 38x6mm with special casted bracket.  Bearing at shaft ends 

	14. Combs/ snatchers 
	Side cover = MS sheet 3mm, 

Snatcher rollers = MS shaft 52 mm dia  with 08Nos splines 

Comb augers = 02 Nos augers pipe shaft dia 38mm, auger sheet thickness 03mm  and auger 175mm dia. Special casted brackets at ends. Comb reinforced at the top with 38 x6 mm angle box and attached with main frame with MS flat 35x 6mm  and MS pipe 39 

Auger guide: MS sheet 3mm thickness  support with side sheet and snatcher roller with 3mm round,   

	15. Main horizontal auger 
	Auger frame : MS angle box 38x6 mm frame welded with the help of MS Plate with main frame and bottom side bolted with MS angle 38x3 mm which rapped the horizontal auger.
Auger cover sheet: MS sheet 3mm perforated at the bottom. 

Auger: MS pipe 50 mm dia. 6mm thickness welded with worm MS  6mm sheet  and total dia of auger is 286 mm. the auger end are special casted.




	16. Vertical conveyor 
	MS sheet 2mm welded with MS angle 38x3mm . Flate belt  with notched flapper MS 2.5 mm sheet.  

	17. Transmission system
	PTO driven, gear box , chain sprocket system and belt pulley system.

PTO to main gear ratio = 1:1.33, 718 RPM

PTO to Snatcher roller ratio = 1:1.25 , 675 RPM

PTO to snatcher auger ratio = 1:0.28   , 150 RPM

PTO to horizontal auger ratio = 1: 0.5 , 270 RPM 

Vertical conveyor RPM = 205 RPM

Ball transfer auger RPM =205 RPM 

	18. Gear boxes connecting shaft
	MS shaft 28.6 connecting the gear boxes with chain sprocket couples. MS cast iron gear box with hardens steel gears.

	19. Mast and toeing hook
	Ms channel box  100x50x6 mm mast. With toe hook of MS rod 25mm dia welded with channel box piece 100x50x 6. 

	20. Ball carrying hopper 
	MS angle 35x 3 mm frame, MS flate 25x 3mm, MS Sheet  3mm at one side, other three side of MS square mesh of 25 mm, with 1.5 mm wire dia. Reinforced with MS flate 25 x3mm at middle of the mesh of the hopper frame.   

	21. Hydraulic jack 
	02 No hydraulic jack to transfer the ball from hopper.  Jack frame of MS channel 78x40x05 mm and 66 x 28x 03mm welded with main frame. Hopper pivoted with MS channel box 66x28x3 mm closed with MS flat 66 x 3 mm.

	22. Transportation system
	MS rectangle box 100x50x06mm welded with main frame at rear end. The other side welded with MS plate 10mm and bolted with axel welded plate. Axel pipe of 60 mm dia. With 6mm thickness. MS shafts end s with hub

	23. Wheels and tyres
	02 Nos type along with Rims of 6.00-16.

	24. Belts pulleys
	Cast iron single groove and B- type belts

	25. Bearing
	Sealed with grease filling facility according to shaft size


MISCELLANEOUS

	26. Paint
	Double coat with primer after surface finish

	27. Nuts and Bolts
	To be tightened with spring washers

	28. Bearings (New)
	NTN,SKF,NSK or equivalent

	29. Lubrication
	Filled with proper lubrication of PSO lubricant of requisite grade and quantity

	30. Minor modifications
	To be carried out free of cost if required

	31. Warranty
	Free : 1 year for parts and service 

Extended: 5 year for parts supply on payment
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SOLAR PANEL SYSTEM (25KW)
	Sr. # 
	Name of Items 
	Specifications/Details
	Quantity

	01
	Solar Panels
	Solar Panels 250 / 300 Watts , Operating Temperature -10 to 85 Degrees Celsius,
	100 / 80

	02
	Solar Inverter
	25kVA, 3 Phase Hybrid  

Solar Power Inverter (Single Cabinet), With synchronizing system, MPPT  Range @ operating Voltage = 60 to 115 V DC, Priority base and load Sharing feature, Input Voltage 440V AC, Out Put 440V AC, Power Factor 0.8, Frequency 50 hz, Voltage Waveform Pure Sine Wave,, Operating temperature -15 to 60 Degree Celsius. Efficiency 93%.
	01

	03
	Batteries

OR

Dry Cell
	200AH, 12 V AGM/VRAL Maintenance

Free Batteries. (Dry )          OR

600 AH, 2 Volts, 
	40

24

	04
	Battery Rack
	Battery Rack for 200Ah, 12 V Battery (for 40 batteries) or 600 AH, 2 Volts Cell (24 Cell)
	02 Set

	05
	Panel Mounting

Structure
	Galvanized Iron (Imported) rust proof 
	01 Set

	06
	Connecting Wires DC
	25mm Single Core, Pure 99.99% Copper 
	R/FT

	07
	Combining & Safety Box
	Built-in Safety instruments for lighting & Combining of Solar panel Cables (Imported)
	01

	08
	AC/DC Inverter
	1.5 Tons
	01 No.

	09
	Services
	Commissioning and Installation of Solar System
	02 years


LABORATORY REFERIGERATOR (2 – 8oC)

TECHNICAL SPECIFICATIONS:
	Capacity
	=
	410L

	Temperature Range
	=
	2oC ~   8oC

	Ambient Temperature
	=
	16oC ~ 32oC

	Cooling Performance
	=
	5°C

	Climate Class
	=
	N

	Controller
	=
	Microprocessor

	Display
	=
	Digital display

	Compressor
	=
	1pcs

	Cooling Method
	=
	Air Cooling

	Defrost Mode
	=
	Automatic

	Refrigerant
	=
	R600a

	Data Logging / Interval/ Recording Time USB
	=
	Record every 10 min/2years

	Access Port
	=
	1pc. Ø 25 mm

	Door Lock with Key
	=
	Yes

	Door
	=
	1

	External Material
	=
	Powder coated material

	Internal Material
	=
	HIPS

	Backup Battery
	=
	Yes

	Temperature
	=
	High/Low temperature, High ambient temperature, Condenser high temperature

	Alarm
	=
	Sensor error, USB data log failure, Door ajar, Remote alarm

	Type
	=
	Vertical

	External Size(W*D*H)
	=
	660*680*2000mm

	Power Supply
	=
	220±10/50(V/HZ)


FREEZER -25°C

TECHNICAL SPECIFICATIONS

	Capacity
	=
	280 Liters

	Temperature Range
	=
	10oC ~ 25oC

	Ambient Temperature
	=
	16oC ~ 32oC

	Cooling Performance
	=
	25°C

	Cooling Method
	=
	Direct Cooling

	Controller
	=
	Microprocessor

	Display
	=
	Digital display

	Access Port
	=
	1pc. Ø 25 mm

	Defrost Mode
	=
	Manual

	Door Lock with Key
	=
	Yes

	Temperature
	=
	High/Low temperature

	System
	=
	Door ajar

	Type
	=
	Vertical

	External Size(W*D*H)
	=
	710*650*1800mm

	Power Supply
	=
	220±10/50(V/HZ)


LAMINAR AIR FLOW CABINET

TECHNICAL SPECIFICATIONS:

	External Size（W*D*H)
	=
	1300*820*2040mm

	Internal Size（W*D*H)
	=
	1200*500*570mm

	Work Surface Height
	=
	750mm

	Display
	=
	LCD Display

	Airflow Velocity
	=
	Average of 0.3~0.5m/s

	Material Main Body
	=
	Cold-rolled steel with anti-bacteria powder coating

	Work Table
	=
	304 stainless steel

	Side and Front Window
	=
	5mm toughened glass, anti-UV

	Pre-filter
	=
	Polyester fiber, washable

	HEPA Filter
	=
	99.999% efficiency at 0.3um

	Noise
	=
	<65dB

	Front Window
	=
	Motorized 

	Max Opening
	=
	430mm

	LED Lamp
	=
	12W*1

	UV Lamp
	=
	30W*1  (Emission of 253.7 nanometers)

	Consumption
	=
	400W 

	Waterproof socket  
	=
	Two, total load≤500W

	Caster
	=
	Universal caster with leveling feet

	Power Supply
	=
	AC220V±10%, 50/60Hz; 110V±10%, 60Hz

	Standard Accessory
	=
	LED lamp, UV lamp*2, Base stand, Gas Tap, Waterproof socket*2, Water Tap

(only for BBS-H1800)

	Optional Accessory
	=
	Electric height adjustable base stand


Temperature Controlled Shaking Incubator
Technical Specifications:

	Temperature Range
	=
	12 °C below Ambient to 60 °C

	Temperature Range Accuracy
	=
	±1.0°C at 37°C

	Temperature Range Increment
	=
	±0.1°C

	Temperature Range Control
	=
	Microprocessor Digital PID Control

	Speed range
	=
	30 to 300 rpm

	Speed range Accuracy
	=
	±1rpm

	Speed range Increment
	=
	1rpm

	Time range
	=
	Continues or up to 47h 59 min

	Time range Accuracy
	=
	±1%

	Motor
	=
	Plate Type Brushless DC Motor

	Drive Systems
	=
	Beltless Direct Drive

	Orbit Diameter
	=
	25 mm

	Operating Panel
	=
	Touch Button

	Chamber Dimensions
	=
	550(W) x 790(D) x 555(H) mm

	Platform Size
	=
	450(W)x450(D)mm

	Capacity to Hold
	=
	250 ml x 23 ea

	Power
	=
	220 V


Ultra Pure Water Purification System

Technical Specifications:

	Frequency
	=
	50/60 Hz

	Feed water Connector
	=
	3/4 in. NPT

	Product Water Type
	=
	Type 1 and 2

	TOC Monitor with UV Intensity Monitoring
	=
	Yes

	Resistivity Type 1
	=
	18.2 Mohm.cm at 25°C; Type 2: 10 to 15 Mohm.cm at 25°C ( Conductivity Type 1: 0.055μS/cm, Type 2: 0.067 to 0.1μS/cm

	Feed water Source
	=
	Tap

	Flow Rate
	=
	0.6 L/min

	Total Organic Carbon
	=
	1 to 5 ppb

	Endotoxin Concentration
	=
	0.005 EU/mL

	Biological Information
	=
	Water should be free from DNase, RNase, Microorganisms


GEL DOCUMENTATION SYSTEM

Technical Specifications:
	Sensor
	=
	1/3 inch

	Resolution
	=
	5 million pixels

	Image depth
	=
	12/16 bit

	Grey scales
	=
	4,096/65,536

	Dynamic range
	=
	3.6 - 4.8

	Lens Manual zoom
	
	6.5 - 39, F1.4

	Maximum viewing area
	
	20 x 20cm

	Illumination White Epi overhead
	
	Yes

	UV Trans illuminator
	
	302 nm

	Image capture
	
	Yes

	Data types
	
	SGD, BMP, TIFF and JPEG

	Image analysis
	
	Yes

	Dimensions (h x d x w) cm
	
	62 x 37.5 x 40


	S.No
	Model
	Features
	Specification

	1
	CI-340

-Handheld Photosynthesis system

(https://cid-inc.com/plant-science-tools/photosynthesis-measurement/ci-340-handheld-photosynthesis-system/)


	· Lightweight and optimized for single-handed operation

· Stable analyzers for accurate CO2 and H2O measurements

· Accommodates open and closed system measurements

· Infrared, non-contact leaf temperature sensor

· Ten interchangeable chambers customized for different leaf types

· Custom soil respiration chamber

· Control modules for light, temperature control, CO2 / H2O supply and chlorophyll fluorescence measurement

· Chlorophyll fluorescence and photosynthesis measured simultaneously
	Main Unit:
On board IRGA for CO2 Analysis, H2O Analysis with humidity sensor capacitor, 
Flow Control, Pump, Display and Key Board, 
Leaf Chambers (LC1, LC3) attachment ports and Battery.

Display:
LCD 40 x 6 characters or 320 x 64 pixel

Data Storage:
4 MB Internal FLASH RAM

Power Supply:
7.2 VDC, 4400 mAh for 5 hours continuous use,
AC Adapter / Battery Charger 

Dimens:
44 cm x 5.5 cm x 5 cm



	2
	CCL-DZ-10Z

Water Distiller

(chinacaremedical.com)
	· High quality stainless steel.
· Condensing coil structure
· 10 L volume of water
· Evaporative cooling water return barrel to save water resources. 
· Release valve barrel 
· Dry automatic cut off heating power
· Copper tube immersion heating, high thermal efficiency, long service life.
	Classification: China Care Medical, 10 L Stainless Steel Electric Distilled Water Device Distiller

Voltage: 220V

Heating power: 7.5KW

Water Discharge = 10 L/hr

Dimens: 42*38*90


	S.No.
	Model
	Features
	Specification

	1


	Olympus SZX7 Stereo Microscope

(With complete System and C-mount compatible with Canon EOS 6D Mark II Camera)

https://www.olympus-ims.com/en/microscope/szx7/#!cms[focus]=cmsContent11272

	· 7:1 Zoom ratio.

· Curved ultra-slim stand with contoured base plates. 

· The Galilean Optical System (0.8x -5.6x zoom range).

· Superior Performance from a Choice of Eight Interchangeable Objectives.

· Ultra-thin and eco-friendly LED stands provide energy-efficient trouble-free usage.

· Single or double interlock and ring light.

· Coaxial Reflected Illumination System.

· A long-lasting ring light illuminator with minimal thermal effect and superior brightness.

· Universal Stand and Digital Imaging
· Recording and Storage of Digital Images
	Weight: 4.5 kg (in Standard Configuration)

Dimensions (W x D x H): 194 mm x 253 mm x 403 mm

Observation Tube: Binocular/Trinocular/Tilting Trinocular Observation Tube

Zoom Body:  7 (0.8x-5.6x)

Total Magnification: 4.0x-336x*1    

Lens: 0.5X & 1X



	2
	Nikon SMZ745 Stereo Microscope (with LED Light System) 

https://www.nikonmetrology.com/en-gb/industrial-microscopes/stereo-microscopes-smz745-745t
	· With Greenough optical system

· Strong build quality and special surface treatments

· Effective electrostatic discharge (ESD) protective coating

· A streamlined shape for enabling maximum ergonomic advantages

· Schott & Photonic that providers of LED and a full range of dedicated microscopy illumination systems
	Total magnification: 3.35-300x
Eyepiece tube: Fixed type
Eyepiece inclination: 45°

Eyepieces (with diopter adjustment): C-W 10xB (F.N. 22), C-W 15x (F.N. 16), C-W 20x (F.N. 12.5), C-W 30x (F.N. 7)

Interpupillary distance adjustment: 52-75 mm

Zooming ratio: 7.5:1 (approx.)

Zooming range: 0.67-5x

Auxiliary objectives: G-AL 0.5x (W.D. 211 mm), G-AL 0.7x (W.D. 150 mm),
G-AL 1.5x (W.D. 61 mm), G-AL 2x (W.D. 43.5 mm)

Working distance: 115 mm

Vertical tube: Built-in C-mount 0.55x magnification lens (F.N. 11), compatible with 2/3 in. or smaller CCD

	3


	Canon EOS 6D Mark II DSLR Camera (With micro lenses and Power Battery)

https://www.usa.canon.com/internet/portal/us/home/products/details/cameras/eos-dslr-and-mirrorless-cameras/dslr/eos-6d-mark-ii
	· Optical Viewfinder with a 45-point All Cross-type AF System

· A 26.2 Megapixel full-frame CMOS sensor (approx. 35.9mm x 24.0mm)

· Capable of sensitivities ranging from ISO 100 to ISO 40000 (expandable to L: 50 and H2: 102400)

· Dual Pixel CMOS AF with Phase-detection & Full HD 60p

· DiG! C 7 Image Processor

· Vari-angle Touch Screen, 3.0-inch LCD

· Built-in Wi-Fi Connectivity, Built-in NFC Capability, Built-in Bluetooth Capability, Built-in GPS Capability

· High-Speed Continuous Shooting at up to 6.5 fps

· Dust & Water-resistant

· The sensor captures images of 6240 x 4160 pixels with a pixel size of 5.67 µm square for outstanding detail and a superb signal-to-noise ratio,

· Compact and lightweight design
	Type: Digital AF/AE single-lens reflex camera

Recording Media: 
· SD/SDHC/SDXC memory cards

· SD speed class-compatible

· UHS speed class-compatible

· High-speed writing is supported when a UHS-I compatible SD card is used.

· Compatible with Eye-Fi cards.

· Multimedia cards (MMC) cannot be used (card error will be displayed).

Image Format: Approx. 35.9 x 24.0mm (Full-frame)

Compatible Lenses: Canon EF lenses (excluding EF-S and EF-M lenses)

Lens Mount: Canon EF mount


	Sr.no
	Model
	Features
	specification

	1
	Nikon Microscope ECLIPSE Ci-E
	Optical system
	CFI60 Infinity Optical System

	
	
	Illumination
	High luminescent White LED Illuminator
Automatic intensity reproduction function

	
	
	Controls
	Image capture button

Nosepiece rotating buttons

Remote control pad

	
	
	Eyepieces

(F.O.V. mm)
	CFI 10X (22)

CFI 12.5X (16)

CFI 15X (14.5)

CFI UW 10X (25)

	
	
	Focusing
	Coaxial Coarse/Fine focusing, Focusing stroke: 30 mm, Coarse: 9.33 mm/rotation, Fine: 0.1 mm/rotation, Fine movement scale 1μm, Coarse motion torque adjustable, Refocusing function

	
	
	Tubes
	C-TB Binocular Tube

	
	
	F.O.V. 22 mm

(Eyepiece/Port)
	C-TE2 Ergonomic Binocular Tube (Eyepiece: Port = 100:0, 50:50) via optional C-TEP2 DSC Port, C-TEP3 DSC Port C-0.55X

Inclination angle: 10-30 degree, Extension: up to 40 mm

	
	
	F.O.V. 25 mm

(Eyepiece/Port)
	F-CTF Trinocular Tube F (Eyepiece: Port = 100:0, 0:100)

TC-TT Trinocular Tube T (Eyepiece: Port = 100:0, 20:80, 0:100)

	
	
	Nosepieces
	Motorized Sextuple Nosepiece with Analyzer Slot (Within main body)

	
	
	Condensers (NA)

Motorized
	CI-C-E Motorized Swing-out Condenser (0.9/0.22)

Focusing stroke: 27 mm

	
	
	Condensers

(NA)

Manual
	C-AB Abbe Condenser

C-AR Achromat Condenser

C-DO Darkfield Condenser Oil

C-DD Darkfield Condenser Dry

C-PH Phase Contrast Turret Condenser

C-AA Achromat/ Aplanat

C-SA Slide Achromat Condenser 2-100X

C-SW Swing-out Achromat Condenser 1-100X

C-SWA Swing-out Achromat Condenser 2-100X

C-LAR LWD Achromat Condener

	
	
	Observation
	Brightfield, Epi-fluorescence, Darkfield, Phase contrast, Simple polarizing, Sensitive color polarizing

	
	
	Epi-fluorescence attachment
	CI-FL-2 Epi-fluorescence Attachment (4 filter cubes mountable)

D-FL-2 U-EPI Epi-fluorescence Attachment

	
	
	Epi-fluorescence attachment
	CI-FL-2 Epi-fluorescence Attachment (4 filter cubes mountable)

D-FL-2 U-EPI Epi-fluorescence Attachment (6 filter cubes mountable, Terminator mechanism)


	
	
	Epi-fluorescence light source
	D-LEDI Fluorescence LED Illumination system

C-HGFI/HGFIE HG Precentered Fiber Illuminator Intensilight (130W)

	
	
	Power consumption
	13W (Brightfield configuration)

	i
	Intuitive camera
DS Ri2 
	Compact, high-performance, budget-friendly, C-mount camera
	16.25 megapixels
Large format CMOS sensors 
High-resolution images. 

	II
	tablet PC
NIS-Elements L
	
	Split screen display
Camera information: Histogram and metadata for the image are displayed.

Full screen: Image can be displayed across the entire screen.

Saving: Displayed image is saved with a new file name.


